City of Slidell

Cross Connection

Control Program

Notice to all Contractors, Developers, Plumbers, or any other

Person/s connecting to the City of Slidell Water System

A Cross Connection Control Permit must be obtained at the

 Office of Building and Safety prior to connecting to the City’s Water System.

1. A Cross Connection Control Permit shall be obtained for each Backflow Device installed.
2. Thermal Expansion Devices shall be installed in accordance with the

 Louisiana State Plumbing Code when installing Backflow Devices.

1. All Backflow Devices shall be installed by a licensed plumber and as per Louisiana State Plumbing Code requirements.
2. All Backflow Devices shall be tested by a State Certified Water Supply Protection Specialist (WSPS) and a copy of the test results shall be provided to the City prior to the start-up of any water service.
3. The following are City recommended devices:

|  |  |
| --- | --- |
| Residential Irrigation (Recommended Devices) | Commercial (Recommended Devices) |
| Watts Series LF009 Reduced Pressure Assemblies | Watts Series LF009 Reduced Pressure Assemblies  |
| Watts Lf008PCQT Vacuum Breakers | Watts 957 Reduced Pressure Assemblies |
|  | Watts LF007 Double Check Valve Assemblies |
|  | Watts Series 709DCDA Double Check Valve Assemblies (Fire Line) |
|  | Watts Series 757DCVA Double Check Valve Assemblies (Fire Line) |

NOTE: Proper Backflow Device selection is crucial to insure the protection of the City’s water system. Should you have questions concerning device selection or need any information about Cross Connection Control please contact us at the number listed below.

City of Slidell Office of Public Utilities 985 646-4291 – Fax 985 646-4238

**NEW CONSTRUCTION**

**WATER TAP AND METER INSTALLATION**

**BEFORE SUBMITTING APPLICATION (in person):**

* Complete the top portion of the New Account Commercial Application - New Construction Form.
* Complete Utility Connection Request Form. (Tap and Meter rates are included in packet)
* The bottom portion of the Utility Connection Request Form **must be signed by the Planning Department** (250 Buscaren Street, Suite 203).
* Picture I.D. and is required in order to process your application.
* Prior account balances must be current before application is processed .
* Billing will be activated once the meter is installed in the field.
* NOTE: PUBLIC OPERATION WILL EVALUATE EACH WATER / SEWER TAP OR INSTALLATION OF METERS TO DETERMINE IF UTILITY EXTENSION FEES ARE NECESSARY.

** UTILITY CONNECTION REQUEST FORM**

**Date: \_\_\_\_\_\_\_\_\_\_\_\_\_**

Name/Contractor: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Installation Address: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Telephone No. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Contact Address: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Request Connection To: **WATER** \_\_\_\_\_\_\_\_\_\_ **SEWER** \_\_\_\_\_\_\_\_\_\_ Number of Tenant Spaces: \_\_\_\_\_\_\_\_\_\_

|  |  |  |
| --- | --- | --- |
| ITEM | SIZE | FEE |
| Water Tap /Connection |  |  |
| Water Tap Work Request Number (Public Operations) | # | \*\*\*\*\*\*\* |
| Water Meter |  |  |
| Water Meter Work Request Number (Public Operations) | # | \*\*\*\*\*\*\* |
| Sewer Use Tax ($850.00) |  |  |
| Sewer Use/Tap Work Request Number (Public Operations) | # | \*\*\*\*\*\*\* |
| Set-Up Fee ($60.00) |  |  |
| Cross Connection Fee Residential Only. ($50.00) |  |  |
| Cross Connection Fee Residential Irrigation OnlyMust obtain a Cross Connection Control Permit at the Building and Safety Office. | Reviewed atBuilding & Safety | Fees Collected atBuilding & Safety |
| Cross Connection Fee CommercialMust obtain a Cross Connection Control Permit at the Building and Safety Office. |  Reviewed atBuilding & Safety | Fees Collected atBuilding & Safety |
| Cross Connection Fire Sprinkler CommercialMust obtain a Cross Connection Control Permit at the Building and Safety Office. | Reviewed atBuilding & Safety | Fees Collected atBuilding & Safety |
| NOTE: A PERMIT IS REQUIRED FOR EACH CROSS CONNECTION CONTROL DEVICE. Please refer to the Cross Connection Control Information Sheet. |  \*\*\*\*\*\*\*\*\*\* |  \*\*\*\*\*\*\*\*\*\* |

 TOTAL \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\*\*\*\**Prior account balances must be current before application is processed*\*\*\*\*

**ADMINISTRATION USE ONLY**

**PLANNING DEPT**. AUTHORIZATION: YES\_\_\_\_\_\_ NO\_\_\_\_\_\_

SIGNATURE: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ DATE\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

# WATER TAP AND WATER METER RATES

The water connection from the system to the property line shall be made by the city at the following rates:

 Size of **Tap** Cost of Tap

 ¾ ” $ 625.00

 1” $ 725.00

 2” $ 775.00

 3” $ 1300.00

 4” $ 1700.00

 6” $ 2000.00

 8” $ 4000.00

Cost of **Meters** with Couplings

 ¾ ” $ 400.00

 1” $ 600.00

 2” $ 1100.00

 3” $ 4400.00

 4” $ 5400.00

 6” U. L. Fireline Meter $ 10800.00

 8” U. L. Fireline Meter\*\*

\*\*To be determined by the City and is dependent upon location.

The Sewer Connection Tax Fee shall be $850.00

***SET-UP FEE*** *--* ***$60.00***

**NOTE**: AFTER YOU HAVE REQUESTED YOUR TAPS AND OR METERS YOUR APPLICATION IS TURNED OVER TO PUBLIC OPERATIONS FOR INSTALLATION. IF YOU HAVE ANY QUESTIONS OR CONCERNS ABOUT THE INSTALLATION ***PLEASE CALL PUBLIC OPS AT: 985-643-6140***